{"text_format":"1","workbook":"xlsx","n_sheets":1,"sheets":["Motorisation"],"not_rendered":{"charts":0,"images":14,"macros":1,"external_links":0,"defined_names":114,"comments":1,"pivot_tables":0},"unopened":[],"bounds":{"document_bytes":16777216,"sheet_cells":100000,"rows_first":2000,"rows_last":500,"rows_between":2000,"halvings":0,"cell_chars":16384,"cell_head_chars":4096},"cells_cut":0,"cells_raw":0,"read":"whole","date_system":"1900"}

{"sheet":"Motorisation","index":0,"n_rows":37,"n_cols":19,"rows_kept":37,"cut":false,"hidden":false,"merged":[[11,8,11,9],[6,8,6,9],[5,8,5,9],[8,8,8,9],[9,8,9,9],[0,3,0,15],[0,1,0,2],[29,8,29,11],[2,8,2,11],[2,1,2,2],[2,4,2,5],[14,4,14,5],[17,4,17,5],[7,8,7,9],[10,8,10,9],[3,8,3,9],[4,8,4,9],[12,9,13,9],[12,10,13,10],[12,11,13,11],[18,1,18,2]]}
[null,"First 162",null,"La plupart des formules de cet onglet sont tirées du fichier de Franck A. (CalculMotorisationSimplifiée.xsl), formules et calculs vérifiés tous ok le 14/07/2015"]
[]
[null,"moteur",null,null,"accu",null,null,null,"Vérifications",null,null,null,null,"Boucher ",{"$f":"O4/(12^5*1000^3)","v":4.0187757201646094E-15}]
[null,"Type de moteur",3.5,null,"Type d'accu",3.7,null,null,"KV du moteur chosi",null,700,null,null,"K = ",{"$f":"F33","v":1}]
[null,"Rendement",85,null,"Nombre d'éléments",4,null,null,"Masse du moteur choisi (g)",null,200]
[null,"Puissance massique (W/kg)",200,null,"Etat de l'accu","1/3 du vol",null,null,"Intensité max du moteur choisi (A)",null,45]
[null,"Puissance moteur min (W)",{"$f":"ROUND((Puissance_Massique_Moteur*(O7/1000)),0)","v":354},null,"Tension moy calculée (V)",{"$f":"F4*F5","v":14.8},null,null,"Puissance max du moteur choisi (W)",null,665,null,null,"Masse du modèle (g)",1770]
[null,"Puissance moteur sécu (W)",{"$f":"ROUND(((((Puissance_Massique_Moteur*(O7/1000))*1.02)*100)/Rendement_Moteur),0)","v":425},null,"Ajustement de la tension (V)",14.8,null,null,"Capacité de l'accu choisi (mAh)",null,4500,null,null,"Masse de l'ESC (g)",70]
[null,"Masse moteur min (g)",{"$f":"ROUND(C8/C4,0)","v":121},null,"Taux de décharge max (C)",35,null,null,"Intensité de décharge constante théorique (A)",null,{"$f":"Capacite_Accu_Choisie*Taux_Decharge_Accu/1000","v":157.5},"A",null,"Surface alaire (dm²)",42]
[null,"Intensité min moteur (A)",{"$f":"ROUND((F10*1.02),1)","v":29.3},null,"Intensité moyenne (A)",{"$f":"ROUND(C8/Tension_Moyenne,1)","v":28.7},null,null,"Intensité de décharge constante conseillée (A)",null,{"$f":"I_Const_Theorique*(2/3)","v":105},"A",null,"Masse totale du modèle (g)",{"$f":"Masse_modele+Masse_Reelle_Accu+Masse_Moteur_Choisie+Masse_ESC","v":2500}]
[null,"Intensité sécur moteur (A)",{"$f":"ROUND(F11*1.02,1)","v":44},null,"Intensité max (A)",{"$f":"ROUND(F10*(3/2),1)","v":43.1},null,null,"Masse calculée de l'accu nu (g)",null,514.28571428571433,"g",null,"Charge Alaire (g/dm²)",{"$f":"O10/O9","v":59.523809523809526}]
[null,"Puissance moteur restituée",{"$f":"ROUND(F10*Tension_Moyenne*0.98*(Rendement_Moteur/100),0)","v":354},null,"Capacité min (mAh)",{"$f":"ROUNDUP((F11/F9)*1000,0)","v":1232},null,null,"Masse réelle de l'accu choisi (g)",null,460,null,null,"Cz aile choisi",0.3]
[null,"Kv",700,null,"Masse accu mini nu (g)",198.62857142857143,null,null,null,"Hélice inférieure","hélice choisie","hélice supérieure"]
[null,"Régime théorique à vide",{"$f":"Tension_Moyenne*C13","v":10360}]
[null,"Régime standard en charge",{"$f":"C14*0.83","v":8598.7999999999993},null,"ESC",null,null,null,"Diamètre (pouces)",{"$f":"ROUNDDOWN(F19,0)","v":12},12,{"$f":"ROUNDUP(F19,0)","v":13},null,null,"km/h","m/s"]
[null,null,{"$f":"(((C15*F20*2.54)/100)/1000)*60","v":78.081380763124542},null,"Intensité constante minimum",{"$f":"C10*1.2","v":35.159999999999997},null,null,"Pas (pouces)",{"$f":"ROUNDDOWN(F20,0)","v":5},6,{"$f":"ROUNDUP(F20,0)","v":6},null,"Vitesse moy palier",{"$f":"(SQRT((2*9.81)/1.293)*SQRT((Charge_Alaire/10)/Cz_AileChoisi))*3.6","v":62.465104610499637},{"$f":"O16/3.6","v":17.351417947361011}]
[null,null,{"$f":"C16*0.8","v":62.465104610499637},null,null,null,null,null,"Rapport Pas/Diamètre",{"$f":"J16/J15","v":0.41666666666666669},{"$f":"K16/K15","v":0.5},{"$f":"L16/L15","v":0.46153846153846156},null,"Coefficient de portance max",0.8]
[null,"Mes hélices:","K",null,"Hélice théorique",null,null,null,"Régime à vide",{"$f":"Tension_Moyenne*K4","v":10360},{"$f":"Tension_Moyenne*Kv_Choisi","v":10360},{"$f":"Tension_Moyenne*K4","v":10360},null,"Vitesse décrochage",{"$f":"4.56*SQRT(Charge_Alaire/Czprofildecrochage)","v":39.333736882514188},{"$f":"O18/3.6","v":10.926038022920608}]
[null,"les hélices vérifiées sont en rouge",null,null,"Diamètre (pouces)",{"$f":"(C12/(O3*F20*C15^3))^(1/4)","v":12.348602750215003},null,null,"Régime standard",{"$f":"J18*0.83","v":8598.7999999999993},{"$f":"K18*0.83","v":8598.7999999999993},{"$f":"L18*0.83","v":8598.7999999999993},null,"Vitesse air brassé",{"$f":"Vitesse_Moyenne_Palier/0.8","v":78.081380763124542},{"$f":"O19/3.6","v":21.689272434201261}]
[null,null,null,null,"Pas (pouces)",{"$f":"Vitesse_Air_Brasse/((2.54*60/100/1000)*Regime_Standard)","v":5.9583316059303453},null,null,"Puissance à l'arbre (W)",{"$f":"Coefficient_K*(J16/12)*((J15/12)^4)*((J19/1000)^3)","v":264.91240881261325},{"$f":"Coefficient_K*(Pas_Helice_Libre/12)*((Diametre_Helice_Libre/12)^4)*((K19/1000)^3)","v":317.89489057513589},{"$f":"Coefficient_K*(L16/12)*((L15/12)^4)*((K19/1000)^3)","v":437.85667292228271}]
[null,null,null,null,"Rapport Pas/Diamètre",{"$f":"F20/F19","v":0.48251059058698803},null,null,"Traction statique (g)",{"$f":"(28.35*(J16)*(J15)^3*J19^2*10^-10)*Coeff_Traction","v":1811.1002948559355},{"$f":"(28.35*(Pas_Helice_Libre)*(Diametre_Helice_Libre)^3*K19^2*10^-10)*Coeff_Traction","v":2173.3203538271232},{"$f":"(28.35*(L16)*(L15)^3*L19^2*10^-10)*Coeff_Traction","v":2763.1856581933966}]
[null,null,null,null,"Coeff de traction",1,null,null,"Vitesse air brassé (km/h)",{"$f":"0.001524*$J$19*J16","v":65.52285599999999},{"$f":"0.001524*$K$19*Pas_Helice_Libre","v":78.6274272},{"$f":"0.001524*$L$19*L16","v":78.6274272},null,null,null,null,null,"Régime standard",{"$f":"K19*Gaz/100","v":8598.7999999999993}]
[null,"6x4,5 rouge aliexpress",1.28,null,"Régime à vide",{"$f":"Tension_Moyenne*KV","v":10360},null,null,"Intensité nécessaire (A)",{"$f":"J20/Tension_Moyenne/0.98/Rendement_Moteur*100","v":21.48797969019607},{"$f":"K20/Tension_Moyenne/0.98/Rendement_Moteur*100","v":25.785575628235286},{"$f":"L20/Tension_Moyenne/0.98/Rendement_Moteur*100","v":35.516098838639458},null,"Gestion des Gaz (%)",100,null,null,"Puissance à l'arbre (W)",{"$f":"Coefficient_K*(Pas_Helice_Libre/12)*((Diametre_Helice_Libre/12)^4)*((S22/1000)^3)","v":317.89489057513589}]
[null,"7x4 noire",1.27,null,"Régime standard",{"$f":"F23*0.83","v":8598.7999999999993},null,null,"Puissance consommée (W)",{"$f":"J23*Tension_Moyenne","v":318.02209941490185},{"$f":"K23*Tension_Moyenne","v":381.62651929788223},{"$f":"L23*Tension_Moyenne","v":525.63826281186402},null,"Tension moyenne (V)",{"$f":"Tension_Moyenne","v":14.8},null,null,"Traction statique (g)",{"$f":"(28.35*(Pas_Helice_Libre)*(Diametre_Helice_Libre)^3*S22^2*10^-10)*Coeff_Traction","v":2173.3203538271232}]
[null,"SF E 8x3.8",1.8,null,"Puissance à l'arbre (W)",{"$f":"Coefficient_K*(F20/12)*((F19/12)^4)*((F24/1000)^3)","v":353.99999999999994},null,null,"Tension moyenne (V)",{"$f":"J24/J23","v":14.8},{"$f":"K24/K23","v":14.8},{"$f":"L24/L23","v":14.8},null,"Intensité correspondante (A)",{"$f":"(O23/100)*K23","v":25.785575628235286},null,null,"Vitesse air brassé (km/h)",{"$f":"0.001524*$S$22*Pas_Helice_Libre","v":78.6274272}]
[null,"GWS EP DD 8x4",null,null,"Traction statique (g)",{"$f":"(28.35*(F20)*(F19)^3*F24^2*10^-10)*Coeff_Traction","v":2351.835209539172},null,null,"Puissance massique (W/kg)",{"$f":"J20/($O$7/1000)","v":149.66802757774761},{"$f":"K20/($O$7/1000)","v":179.60163309329712},{"$f":"L20/($O$7/1000)","v":247.37665136852129},null,"Puissance consommée (W)",{"$f":"O24*O25","v":381.62651929788223},null,null,"Intensité nécessaire (A)",{"$f":"S23/Tension_Moyenne/0.98/Rendement_Moteur*100","v":25.785575628235286}]
[null,"APC 8x4 E",1.3,null,"Vitesse air brassé (km/h)",{"$f":"0.001524*F24*F20","v":78.081380763124542},null,null,"Vitesse de vol (km/h)",{"$f":"J22*0.8","v":52.418284799999995},{"$f":"K22*0.8","v":62.90194176},{"$f":"L22*0.8","v":62.90194176},null,"Traction statique (g)",{"$f":"(28.35*(Pas_Helice_Libre)*(Diametre_Helice_Libre)^3*O29^2*10^-10)*Coeff_Traction","v":2173.3203538271196},null,null,"Puissance consommée (W)",{"$f":"S26*Tension_Moyenne","v":381.62651929788223}]
[null,"SF Electric Prop 8x4.5",null,null,"Intensité nécessaire (A)",{"$f":"F25/Tension_Moyenne/0.98/Rendement_Moteur*100","v":28.714188378053919},null,null,"Autonomie plein gaz (mn)",{"$f":"Capacite_Accu_Choisie/1000/J23*60*0.95","v":11.936906293569729},{"$f":"Capacite_Accu_Choisie/1000/K23*60*0.95","v":9.9474219113081084},{"$f":"Capacite_Accu_Choisie/1000/L23*60*0.95","v":7.2220769844502977},null,"Puissance à l'arbre",{"$f":"O25*$O$24*0.98*(Rendement_Moteur/100)","v":317.89489057513589},null,null,"Tension moyenne (V)",{"$f":"S27/S26","v":14.8}]
[null,"SF E 9x4.7",1.24,null,null,null,null,null,null,null,null,null,null,"Régime (T/mn)",{"$f":"(O28/(Diametre_Helice_Libre^4*O3*Pas_Helice_Libre))^(1/3)","v":8598.799999999992},null,null,"Puissance massique (W/kg)",{"$f":"S23/($O$7/1000)","v":179.60163309329712}]
[null,"TP Slow Fly  10x4.7 GWS",1.4,null,null,null,null,null,"Turnigy Aerodrive SK3 - 3548-700kv",null,null,null,null,"Vitesse air brassé",{"$f":"0.001524*$O$29*Pas_Helice_Libre","v":78.627427199999929},{"$f":"O30/3.6","v":21.84095199999998},null,"Vitesse de vol (km/h)",{"$f":"S25*0.8","v":62.90194176}]
[null,"GWS EP DD 10x6",0.84,null,null,null,null,null,"Kv annoncé",700,"mesuré",null,null,"Vitesse de vol (km/h)(m/s)",{"$f":"O30*0.8","v":62.901941759999943},{"$f":"O31/3.6","v":17.472761599999984},null,"Autonomie plein gaz (mn)",{"$f":"Capacite_Accu_Choisie/1000/S26*60*0.95","v":9.9474219113081084}]
[null,"APC 11x5.5 E",0.94,null,"Hélices théoriques","K",null,null,"45A"]
[null,"Beech wood 12x5",0.65,null,"toutes",1,null,null,"665W"]
[null,"Cherry wood 12x6",1,null,"APC 9x5",1.1000000000000001,null,null,"177g",null,null,null,null,{"$f":"(2.54*60/100/1000)","v":1.524E-3}]
[null," GWS EP RD 12x6"]
[]
[null,"9x5 Noire HK ",1]